RPS, Technical information, IT-HIST-S3T MCU-079.
--------------------------------------------------------------------------------
Subject: Firmware history for systems S3_MCU (Sentryum LCD display).
A. Pajola, Date: 13/06/2025
--------------------------------------------------------------------------------
Modification category:
N=new feature
I=improvement
B=bug fix
C=critical bug fix
T=technical

--------------------------------------------------------------------------------
FW079-0109: FW079-0109.dfu     [13/06/2025] MD5:[8733c3a81480dfab2936895f8ad2920f] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese, Czech, Polish, Russian
                     Danish, Turkish, Chinese, Swedish
                     
N   - Added Swedish language.

--------------------------------------------------------------------------------
FW079-0108: FW079-0108.dfu     [21/03/2024] MD5:[d7cd751638cabfd589fabd11b2e5ff82] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese, Czech, Polish, Russian
                     Danish, Turkish, Chinese

N   - Added the Danish, Turkish, Chinese languages.
N   - Added alarm codes for signaling specific external alarms
                         [A60] Insulation loss A.C.
                         [A61] Insulation loss D.C.
                         [A62] Fan fault cabinet
                         [A63] External alarm 1"
                         [A64] External alarm 2"

--------------------------------------------------------------------------------
FW079-0107: FW079-0107.dfu     [18/03/2022] MD5:[dc55fff55daa81f3329cdacbbd98a89f] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese, Czech, Polish, Russian

T   - Modified some operating parameters of the display for compatibility with a new manufacturer
      (PCLK,HSYNC,HBP,HFP,VSYNC,VBP,VFP).

--------------------------------------------------------------------------------
FW079-0106: FW079-0106.dfu     [13/10/2021] MD5:[7a4ba6556a969cfe188a7d9c53ae60c1] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese, Czech, Polish, Russian

N   - Added alarm codes for the management of the Energy Manager and BMS:
                         [W09] BMS status - Warning
                         [W10] BMS cmd - Stop charge
                         [W11] BMS cmd - Stop discharge
                         [A53] BMS status - Anomaly
                         [A54] BMS - Communication lost
                         [A55] ENM - Communication lost
                         [F38] BMS status - Fault
                         [L58] BMS status - Lock
N   - Removed the indication of the estimated autonomy time for SuperCaps UPS.
I   - Added the possibility to stop the "Battery autonomy test" from the panel. To stop the test it is
      necessary to press the command button "0 Battery test" in the command panel.
I   - Modified the display of the event log. In the date field the indication of the year has been removed
      and the display of the seconds has been added.
I   - Modified the display of the event log. For events from [E01] to [E32], the "Rise/Fall" indication
      has been removed.

--------------------------------------------------------------------------------
FW079-0105: FW079-0105.dfu     [30/10/2020] MD5:[75BA18C03909C68427D726FFAB41936C] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese, Czech, Polish, Russian

N   - Added the Czech, Polish and Russian languages.
N   - Added management of the warning screen for the "Deep discharge protection status"
      in the models CBT/CBM (CSS).
N   - Added alarm codes [A45] and [A46] for the models CBT/CBM (CSS).
I   - Added alarm code [F61].

--------------------------------------------------------------------------------
FW079-0104: FW079-0104.dfu     [20/02/2020] MD5:[FFBCCF06E2D3B4052CC8E6FD06BB1ABC] Standard production

Supported languages: English, French, German, Italian, Spanish, Portuguese

N   - Added the Portuguese language.
I   - Added in the service messages [W07] and [W08] the visualization of the service
      phone number. To configure the phone number is required the S3Config software
      release 1.0.4 or later (Commands:Set service date:Service phone number).
I   - Added the possibility to disable/enable the configuration of the parameters
      "Output voltage","Output frequency" and "Battery capacity" from the control panel.
      To use this function is required the S3Config software release 1.0.4 or later
      (parameter Service:Enabling panel configuration).
I   - Added the possibility to configure also the Internal Battery Capacity (only
      if this type of configuration is enabled, see the previous point).
I   - In case of output not powered the estimated autonomy time is not longer displayed.
B   - Corrected the display of the power derating percentages in case of nominal
      output voltage lower than 225V
B   - Fixed a problem of scrolling of the Event Log that occured in particular
      cases.

--------------------------------------------------------------------------------
