Note: the system firmware is different for the two cards "2032" and "2143"

System card "2032" uses:

 -> PXP028rev... .hex  

System card "2143" requires "MSFLASH 10.0" or later and uses:
  
 -> PXP2-028rev.... .hex
