DSPFlash 2.02   

Overview
========================================
DSPFlash 2.02 is a flash software to program the boards: 2112(DSP board MHT) 2148(DSP board NXE) 2124(Graphic b/w board) S3T
Requirements
========================================
- x86 or x64 PC System with USB port 
- DSPFlash 2.00.zip 
- FTDI driver
- NET Framework 4.0 or higher

Note
========================================
- NET Framework 4.0 or higher 
	DSPFlash 2.00 requires the Microsoft .NET Framework 4.0 installed on your system to run the application.
  	This can be obtained from the Microsoft Website http://www.microsoft.com/download/en/details.aspx?id=17851&WT.mc_id=MSCOM_EN_US_DLC_DETAILS_121LSUS007996
	If your system does not have .NET 4.0 installed please download the file from the above link. To install,
  	 double click on the dotnetfx.exe and follow the instructions in the wizard. 


- FTDI driver
	DSPFlash 2.02 requires the Windows FTDI driver installed.
 	This can be obtained from the FTDI Website https://www.ftdichip.com/Drivers/VCP.htm FTDI VCP DRIVER EXECUTABLE, 
          Available as a setup executable (Example CDM21228_Setup.exe).
          To install double click on thethe exe file.
  

Package Contents
========================================
DSPFlash 2.02.zip

Installation:
========================================

1. Unpack the file DSPFlash 2.02.zip

2. Launch DSPFlash 2.02.exe



